Current charge state, Cs (kWh), is given by:

Where:

Pc = Battery charge at beginning of session (%)

Uc = Usable capacity of battery (kWh)

d = Duration of charge (hours)

Cr = Charge rate of station (kW)